**INTERCONNECT CONDUIT GENERAL NOTES:**

1. All pull boxes shall be No. 5 and shall be located behind the sidewalk, as shown, or as directed by the Engineer.
2. All conduits shall be 2 inch PVC per the Standard Specifications.
3. The station locations for pull boxes are approximate and shall be verified in the field by the Engineer.
4. All pull boxes and conduits shall be placed within ADOT right-of-way.
5. All conduits shall have a No. 8 AWG bare bond wire installed per Section 732-2.01 of the Standard Specifications.
6. All existing conduit and pull boxes are to remain, unless the plans show otherwise.
7. All pull boxes shall be left in a clean condition, free of dirt and debris, upon completion of the work.
8. All material and installation shall conform to the 2008 Standard Specifications and ADOT’s Traffic Signals and Lighting Standard Drawings.
9. The locations of utilities shown on the plans are approximate. All involved utilities may not be shown on the plans. The Contractor shall be responsible, per Section 730-6 of the Standard Specifications, for contacting all utilities for exact locations prior to any construction activity.