**ROADWAY LIGHTING GENERAL NOTES:**

1. For installation procedures, see ADOT’s Traffic Signal and Lighting Standard Drawings and the 2008 Standard Specifications.
2. The location of utilities shown on the plans are approximate. All involved utilities may not be shown on the plans. The Contractor shall be responsible per Sections 107.15 & 730-6 of the Standard Specifications, for contacting all utilities for the exact location prior to any construction activity.
3. All lighting units shall be installed with the mast arm perpendicular to the lane or ramp on which they are located.
4. For electrical service requirements, contact \_\_\_\_\_\_\_\_\_ of (name of utility company) at \_\_\_\_\_\_\_\_\_\_\_\_\_\_ per Section 107 of the Special Provisions.