**UNDERGROUND CONDUIT NOTES:**

1. All materials and installation shall conform to the 2008 Standard Specifications and the most recent Traffic Signal and Lighting Standard Drawings.
2. All involved utilities may not be shown on the plans. The Contractor shall be responsible per Section 730-6 of the Standard Specifications for contacting all utilities for exact locations prior to any construction activity.
3. All pull boxes shall be left in a clean condition, free of dirt and debris, upon completion of the work.